#include "skeleton.dtsi"

/ {
	compatible = "nvidia,tegra30";

	tegra_car: clock {
		compatible = "nvidia,tegra30-car";
		reg = <0x60006000 0x1000>;
		#clock-cells = <1>;
	};

	apbdma: dma {
		compatible = "nvidia,tegra30-apbdma", "nvidia,tegra20-apbdma";
		reg = <0x6000a000 0x1400>;
		interrupts = <0 104 0x04
			      0 105 0x04
			      0 106 0x04
			      0 107 0x04
			      0 108 0x04
			      0 109 0x04
			      0 110 0x04
			      0 111 0x04
			      0 112 0x04
			      0 113 0x04
			      0 114 0x04
			      0 115 0x04
			      0 116 0x04
			      0 117 0x04
			      0 118 0x04
			      0 119 0x04
			      0 128 0x04
			      0 129 0x04
			      0 130 0x04
			      0 131 0x04
			      0 132 0x04
			      0 133 0x04
			      0 134 0x04
			      0 135 0x04
			      0 136 0x04
			      0 137 0x04
			      0 138 0x04
			      0 139 0x04
			      0 140 0x04
			      0 141 0x04
			      0 142 0x04
			      0 143 0x04>;
		clocks = <&tegra_car 34>;
	};

	gpio: gpio {
		compatible = "nvidia,tegra30-gpio";
		reg = <0x6000d000 0x1000>;
		interrupts = <0 32 0x04
			      0 33 0x04
			      0 34 0x04
			      0 35 0x04
			      0 55 0x04
			      0 87 0x04
			      0 89 0x04
			      0 125 0x04>;
		#gpio-cells = <2>;
		gpio-controller;
		#interrupt-cells = <2>;
		interrupt-controller;
	};

	i2c@7000c000 {
		compatible =  "nvidia,tegra30-i2c", "nvidia,tegra20-i2c";
		reg = <0x7000c000 0x100>;
		interrupts = <0 38 0x04>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car 12>, <&tegra_car 182>;
		clock-names = "div-clk", "fast-clk";
		status = "disabled";
	};

	i2c@7000c400 {
		compatible = "nvidia,tegra30-i2c", "nvidia,tegra20-i2c";
		reg = <0x7000c400 0x100>;
		interrupts = <0 84 0x04>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car 54>, <&tegra_car 182>;
		clock-names = "div-clk", "fast-clk";
		status = "disabled";
	};

	i2c@7000c500 {
		compatible = "nvidia,tegra30-i2c", "nvidia,tegra20-i2c";
		reg = <0x7000c500 0x100>;
		interrupts = <0 92 0x04>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car 67>, <&tegra_car 182>;
		clock-names = "div-clk", "fast-clk";
		status = "disabled";
	};

	i2c@7000c700 {
		compatible = "nvidia,tegra30-i2c", "nvidia,tegra20-i2c";
		reg = <0x7000c700 0x100>;
		interrupts = <0 120 0x04>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car 103>, <&tegra_car 182>;
		clock-names = "div-clk", "fast-clk";
		status = "disabled";
	};

	i2c@7000d000 {
		compatible = "nvidia,tegra30-i2c", "nvidia,tegra20-i2c";
		reg = <0x7000d000 0x100>;
		interrupts = <0 53 0x04>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car 47>, <&tegra_car 182>;
		clock-names = "div-clk", "fast-clk";
		status = "disabled";
	};

	spi@7000d400 {
		compatible = "nvidia,tegra30-slink", "nvidia,tegra20-slink";
		reg = <0x7000d400 0x200>;
		interrupts = <0 59 0x04>;
		nvidia,dma-request-selector = <&apbdma 15>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car 41>;
		status = "disabled";
	};

	spi@7000d600 {
		compatible = "nvidia,tegra30-slink", "nvidia,tegra20-slink";
		reg = <0x7000d600 0x200>;
		interrupts = <0 82 0x04>;
		nvidia,dma-request-selector = <&apbdma 16>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car 44>;
		status = "disabled";
	};

	spi@7000d800 {
		compatible = "nvidia,tegra30-slink", "nvidia,tegra20-slink";
		reg = <0x7000d480 0x200>;
		interrupts = <0 83 0x04>;
		nvidia,dma-request-selector = <&apbdma 17>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car 46>;
		status = "disabled";
	};

	spi@7000da00 {
		compatible = "nvidia,tegra30-slink", "nvidia,tegra20-slink";
		reg = <0x7000da00 0x200>;
		interrupts = <0 93 0x04>;
		nvidia,dma-request-selector = <&apbdma 18>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car 68>;
		status = "disabled";
	};

	spi@7000dc00 {
		compatible = "nvidia,tegra30-slink", "nvidia,tegra20-slink";
		reg = <0x7000dc00 0x200>;
		interrupts = <0 94 0x04>;
		nvidia,dma-request-selector = <&apbdma 27>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car 104>;
		status = "disabled";
	};

	spi@7000de00 {
		compatible = "nvidia,tegra30-slink", "nvidia,tegra20-slink";
		reg = <0x7000de00 0x200>;
		interrupts = <0 79 0x04>;
		nvidia,dma-request-selector = <&apbdma 28>;
		#address-cells = <1>;
		#size-cells = <0>;
		clocks = <&tegra_car 105>;
		status = "disabled";
	};

	sdhci@78000000 {
		compatible = "nvidia,tegra30-sdhci";
		reg = <0x78000000 0x200>;
		interrupts = <0 14 0x04>;
		clocks = <&tegra_car 14>;
		status = "disabled";
	};

	sdhci@78000200 {
		compatible = "nvidia,tegra30-sdhci";
		reg = <0x78000200 0x200>;
		interrupts = <0 15 0x04>;
		clocks = <&tegra_car 9>;
		status = "disabled";
	};

	sdhci@78000400 {
		compatible = "nvidia,tegra30-sdhci";
		reg = <0x78000400 0x200>;
		interrupts = <0 19 0x04>;
		clocks = <&tegra_car 69>;
		status = "disabled";
	};

	sdhci@78000600 {
		compatible = "nvidia,tegra30-sdhci";
		reg = <0x78000600 0x200>;
		interrupts = <0 31 0x04>;
		clocks = <&tegra_car 15>;
		status = "disabled";
	};

	usb@7d000000 {
		compatible = "nvidia,tegra30-ehci";
		reg = <0x7d000000 0x4000>;
		interrupts = <52>;
		phy_type = "utmi";
		clocks = <&tegra_car 22>;	/* PERIPH_ID_USBD */
		status = "disabled";
	};

	usb@7d004000 {
		compatible = "nvidia,tegra30-ehci";
		reg = <0x7d004000 0x4000>;
		interrupts = <53>;
		phy_type = "hsic";
		clocks = <&tegra_car 58>;	/* PERIPH_ID_USB2 */
		status = "disabled";
	};

	usb@7d008000 {
		compatible = "nvidia,tegra30-ehci";
		reg = <0x7d008000 0x4000>;
		interrupts = <129>;
		phy_type = "utmi";
		clocks = <&tegra_car 59>;	/* PERIPH_ID_USB3 */
		status = "disabled";
	};
};
