/*
 * Copyright (C) 2011 Marek Vasut <marek.vasut@gmail.com>
 * on behalf of DENX Software Engineering GmbH
 *
 * January 2004 - Changed to support H4 device
 * Copyright (c) 2004-2008 Texas Instruments
 *
 * (C) Copyright 2002
 * Gary Jennejohn, DENX Software Engineering, <garyj@denx.de>
 *
 * SPDX-License-Identifier:	GPL-2.0+
 */

OUTPUT_FORMAT("elf32-littlearm", "elf32-littlearm", "elf32-littlearm")
OUTPUT_ARCH(arm)
ENTRY(_start)
SECTIONS
{
	. = 0x00000000;

	. = ALIGN(4);
	.text	:
	{
		arch/arm/cpu/arm926ejs/spear/start.o	(.text*)
		*(.text*)
	}

	. = ALIGN(4);
	.rodata : { *(SORT_BY_ALIGNMENT(SORT_BY_NAME(.rodata*))) }

	. = ALIGN(4);
	.data : {
		*(.data*)
	}

	. = ALIGN(4);

	.rel.dyn : {
		__rel_dyn_start = .;
		*(.rel*)
		__rel_dyn_end = .;
	}

	.bss : {
		. = ALIGN(4);
		__bss_start = .;
		*(.bss*)
		. = ALIGN(4);
		__bss_end = .;
	}

	.end :
	{
		*(.__end)
	}

	_image_binary_end = .;

	.dynsym _image_binary_end : { *(.dynsym) }
	.dynbss : { *(.dynbss) }
	.dynstr : { *(.dynstr*) }
	.dynamic : { *(.dynamic*) }
	.hash : { *(.hash*) }
	.plt : { *(.plt*) }
	.interp : { *(.interp*) }
	.gnu : { *(.gnu*) }
	.ARM.exidx : { *(.ARM.exidx*) }
}
