/****************************************************************************
**
** Copyright (C) 2022 The Qt Company Ltd.
** Contact: https://www.qt.io/licensing/
**
** This file is part of the Qt Creator documentation.
**
** Commercial License Usage
** Licensees holding valid commercial Qt licenses may use this file in
** accordance with the commercial license agreement provided with the
** Software or, alternatively, in accordance with the terms contained in
** a written agreement between you and The Qt Company. For licensing terms
** and conditions see https://www.qt.io/terms-conditions. For further
** information use the contact form at https://www.qt.io/contact-us.
**
** GNU Free Documentation License Usage
** Alternatively, this file may be used under the terms of the GNU Free
** Documentation License version 1.3 as published by the Free Software
** Foundation and appearing in the file included in the packaging of
** this file. Please review the following information to ensure
** the GNU Free Documentation License version 1.3 requirements
** will be met: https://www.gnu.org/licenses/fdl-1.3.html.
**
****************************************************************************/

/*!
    \page creator-embedded-platforms.html
    \previouspage creator-desktop-platforms.html
    \nextpage creator-mobile-platforms.html

    \title Embedded Platforms

    You can develop applications for the following embedded platforms:

    \list
        \li \l {Bare Metal}
        \li \l {Boot2Qt}
        \li \l {Generic Remote Linux}
        \li \l {Microcontroller Units (MCU)}
        \li \l QNX
    \endlist

    You must install the tool chain for building applications for the targeted
    embedded platform on the development PC and use the Qt Maintenance Tool to
    install Qt libraries that are built for the platform. You can then add a
    \l{glossary-buildandrun-kit}{kit} with the tool chain and the Qt version
    for the device's architecture. When possible, the Maintenance Tool creates
    suitable kits for you.

    You can connect embedded devices to the development PC to run, debug, and
    analyze applications built for them from \QC.

    \section1 Bare Metal

    You can run and debug applications on small devices that are not supported
    by the generic remote Linux device plugin by using GDB or a hardware
    debugger.

    For more information about developing applications for Bare Metal devices,
    see \l{Connecting Bare Metal Devices}.

    \section1 Boot2Qt

    The Boot2Qt stack can be made to run on a variety of hardware. For
    license holders, tooling is provided to customize the contents of the stack
    as well as to take it into desired production hardware.

    Either Windows 7 or later or Ubuntu Linux 64-bit 12.04 LTS
    or later is required to install and use Boot2Qt.

    The following topics contain more information about developing applications
    for Boot2Qt devices:

    \list
        \li \l{https://doc.qt.io/QtForDeviceCreation/qtee-supported-platforms.html}
            {Reference Target Devices and Development Hosts}
        \li \l{https://doc.qt.io/QtForDeviceCreation/b2qt-installation-guides.html}
            {Installation Guides}
        \li \l{Connecting Boot2Qt Devices}
        \li \l{Specifying Run Settings for Boot2Qt Devices}
        \li \l{Deploying Applications to Boot2Qt Devices}
        \li \l{https://doc.qt.io/qtcreator/creator-overview-qtasam.html}
            {Qt Creator Plugin for Qt Application Manager}
        \li \l{https://doc.qt.io/QtForDeviceCreation/index.html}
            {Qt for Device Creation}
    \endlist

    \section1 Generic Remote Linux

    You must have a tool chain for building applications for embedded Linux
    devices installed on the development PC.

    The following topics contain more information about developing applications
    for generic remote Linux devices:

    \list
        \li \l{Connecting Generic Remote Linux Devices}
        \li \l{Deploying Applications to Generic Remote Linux Devices}
        \li \l{Specifying Run Settings for Linux-Based Devices}
        \li \l{Running on Generic Remote Linux Devices}
        \li \l{https://doc.qt.io/qtcreator/creator-overview-qtasam.html}
            {Qt Creator Plugin for Qt Application Manager}
    \endlist

    \section1 Microcontroller Units (MCU)

    You need the GNU Arm Embedded GCC compiler, libraries, and other GNU tools
    necessary for bare metal software development on devices based on the Arm
    Cortex-M processors.

    The following topics contain more information about developing applications
    for MCUs:

    \list
        \li \l{Connecting MCUs}
        \li \l{Running Applications on MCUs}
        \li \l{https://doc.qt.io/QtForMCUs/index.html}{Qt for MCUs}
    \endlist

    \section1 QNX

    The QNX Neutrino RTOS should provide a few additional command line tools
    and services, as described in \l {Qt for QNX}.

    \note In Qt 6, \QC support for QNX is considered experimental.

    The following topics contain more information about developing applications
    for QNX devices:

    \list
        \li \l{Connecting QNX Devices}
        \li \l{Deploying Applications to QNX Neutrino Devices}
        \li \l{Specifying Run Settings for QNX Devices}
        \li \l{Running on QNX Devices}
        \li \l{Qt for QNX}
    \endlist
*/
