- Qt Creator Documentation
- Set up the uVision IDE
- Qt Creator 20.0.0-beta1

Set up St-Link ◦ Developing for Boot to Qt devices

# Set up the uVision IDE

uVision is an IDE for developing applications for embedded devices. To debug applications, use uVision Simulator, or debug directly on hardware by using St-Link and J-Link.

The Peripheral Registers view in Debug mode shows the current state of peripheral registers. The view is hidden by default.

## uVision Simulator

}

To set preferences for uVision Simulator:

1. Go to Preferences > Devices > Bare Metal.
2. Select Add.
3. Select uVision Simulator.
4. In Name, enter a name for the connection.
5. In Host, select the host name and port number to connect to the debug server provider.
6. In Tools file path, enter the path to the Keil toolset configuration file.
7. In Target device, select the device to debug.
8. In Target driver, select the driver for connecting to the target device.
9. Select Limit speed to real-time to limit the connection speed.
10. Select Apply to add the debug server provider.

## uVision St-Link or JLink Debugger

To set preferences for uVision St-Link or JLink Debugger:

1. Go to Preferences > Devices > Bare Metal.
2. Select Add.
3. Select uVision St-Link or uVision JLink.
4. In Name, enter a name for the connection.
5. In Host, select the host name and port number to connect to the debug server provider.
6. In Tools file path, enter the path to the Keil toolset configuration file.
7. In Target device, select the device to debug.
8. In Target driver, select the driver for connecting to the target device.
9. In Adapter options specify the adapter interface type and speed in MHz.
10. Select Apply to add the debug server provider.

See also How to: Develop for Bare Metal and Developing for Bare Metal Devices.

Set up St-Link ◦ Developing for Boot to Qt devices