Based on MAME 0.152.
Fixes in MAME 0.154 to 0.197 are applied.

cycle_table_rm/pm are changed from dynamic array to static array.
convert char to _TCHAR in disassembler.
mov_r16_rm16 is modified to check limit for NEC PC-9801RA's ITF routine.
