Ascension Ultra  -   mesh information

******************************************COORDINATE SYSTEMS

** Earth position **
Global LONG/LAT:	-14.405	-7.955
Intended Heading (a):	130°
Heading of base:	230° = -130°
Heading of vessel:	220° = 130°+90°

(suffix '(g)' indicates global coordinates, suffix '(l)'
 indicates mesh-local coordinates, suffix '(b)' is for base
 configuration-file coordinates)

* Global 0,0 is in the top left corner of the basefloor mesh

* Global direction is positive to the right and down

* Landing-point to 0,0 offset-vector:	-2700,0,-950(g)

* Transformation matrix for global coordinates to vessel:
	| -1	0	0	|
	| 0	1	0	|
	| 0	0	1	|
  (or just invert the x coordinate)

* Transformation matrix for global coordinates to base:
	| -cos(a)	0	sin(a)	|
	| 0		1	0	|
	| sin(a)	0	cos(a)	|
  (with a=130° and offset -2700,0,-950(g) =>
	-2463.268767,0,-1457.671767(b))


*************************************************************TURNAROUND HANGAR

** Y-axis curviture compensation adjustment **
TA Hangar 1 (rightmost)
-0.02
TA Hangar 2
-0.05
TA Hangar 3
-0.08
TA Hangar 4
-0.12
TA Hangar 5
-0.17

** Offset-vector for hangar 1 (rightmost) **
2242,0,580

** Relevant Mesh Groups **
0 - crane_beam
1 - crane_upper jig
2 - crane_cables
3 - crane_lower jig
4 - +Z main door
5 - -Z main door
6 - +X service door
7 - -X service door

** Rest Positions **
Cross Beam  -65,33,0
Upper Jig   -65,31.5,-9
Cables      -65,30,-9
Lower Jig   -65,28.5,-9

** Animation Data **
CRANEXOFFSET		130.0
CRANEYOFFSET		18.0
CRANEREELUPPERPOINT	31.0
CRANEREELLOWERPOINT	29.0

** Translation Distances **
X axis = 130m
Y axis = 18m
Z axis = 29m 

** Door Animations **
Main Hangar Doors - 30 degree X axis rotation around 0,0,0
End Doors - 6m translation +Y axis

** Spacing between hangars **
266m

** Observation Room Camera Positions **
** (relative to hangar origin)       **
88,22,0
-88,22,0
Cameras point toward 0,0,0 as default

** Crew lounge entrance area **
**(relative to hangar origin)**
72,0,-33
-72,0,-33

**************************************************************** LIGHT STORAGE HANGAR
12 Hangars

** Y-axis curviture compensation adjustment **
TBC

**Offset vector for hangar L1 (rightmost)
855,0,480

** Relevant Mesh Groups **
0 - Access Door Lower
1 - Access Door Upper
2 - Main Door -x
3 - Main DOor +x

** Door Animations **
Main Hangar Doors +x  +45 degree Y axis rotation around 0,0,0
Main Hangar Doors -x  -45 degree Y axis rotation around 0,0,0
Access Doors Lower 3.62m translation +Y axis
Access Door Upper 1.81m transition +Y axis

** Spacing between hangars **
70m


******************************************************** Launch Facility & Mission Control
1 mesh

** Y-axis curviture compensation adjustment **
TBC

**Offset vector for hangar L1 (rightmost)
1463,0,1260

** Relevant Mesh Groups **
0 - Main Door (entrance)
1 - Exit Door (exit to launch tunnel)
2 - Blast Shield
3 - Tunnel Door

** Door Animations **
Main Door +45 degree Z axis rotation around -223,0,0
Exit Door -45 degree Z axis rotation around 0,0,0
Blast Shield -90 degree Y axis rotation around 189.3,0,47.5
Tunnel Door 47m Translation -X axis 

** Spacing between hangars **
N/A


****************************************************************PLACE HOLDER
** Offset-vector
0,0,0
