# setrts

Changes the RTS(Request To Send) status of Tera Term. (version 4.59 or later)

    setrts <flag>

## Remarks

If the connection is not serial connection or flow control is not "none", this command will do nothing.

If <echo flag> is zero, the RTS is turned off.
If <echo flag> is non-zero, the RTS is turned on.

## Example

    ; RTS on
    setrts 1

    ; RTS off
    setrts 0

## See also

- setdtr