# Keyboard setup file

The keyboard setup file assigns keys on PC keyboard for various functions such as VT terminal functions, sending user defined character strings, Tera Term commands and executing macro files.
You can modify key assignments by editing the file. See KEYCODE.TXT for the format of keyboard setup file.

The file name of keyboard setup file to be loaded by Tera Term can be specified as a command line parameter of Tera Term. If you omit the file name extension, the default extension ".CNF" is assumed. If you omit the file name, the default file KEYBOARD.CNF is loaded.

The distribution package contains the following keyboard setup files:

IBMKEYB.CNF
  Sample file for the IBM-PC/AT 101-key keyboard
VT200.CNF
  The location of these keys on VT220 is different from a generic 101(106) keyboard. For example if "End" key is pressed, the key code of "Page up" (when IBMKEYB.CNF is used) is sent.
KEYBOARD.CNF
  Default keyboard setup file (copy of IBMKEYB.CNF at the moment just after the installation)

The installer will copy IBMKEYB.CNF on KEYBOARD.CNF. If you want to use a different key map, copy an appropriate file on KEYBOARD.CNF to meet your need.

## Keyboard Layout

### Editing keypad

Insert | Home | Page Up
Delete | End | Page Down

101 Keyboard

Find | Insert Here | Re- move
Select | Prev Screen | Next Screen

VT200 Keyboard

### Numeric keypad

Num Lock | / | * | -
7 | 8 | 9 | +
4 | 5 | 6
1 | 2 | 3 | Enter
0 | .

101 Keyboard

PF1 | PF2 | PF3 | PF4
7 | 8 | 9 | -
4 | 5 | 6 | ,
1 | 2 | 3 | Enter
0 | .

VT200 Keyboard

# ABOUT THE KEYBOARD SETUP FILE

## FORMAT OF THE KEYBOARD SETUP FILE

Each key or key combination has a unique key code, which is called "PC key code".

The keyboard setup file has six sections.

- [VT editor keypad]
- [VT numeric keypad]
- [VT function keys]
- [X function keys]
- [Shortcut keys]
- [User keys]

### [VT editor keypad] section

In this section, VT editor keys are assigned to PC keys.

    	Format:
    		<VT editor key name>=<PC key code>

    	where:

    	<VT editor key name>
    		Up, Down, Right, Left, Find, Insert, Remove, Select,
    		Prev, Next

    	  <PC key code>
    		PC key code (decimal number)

    	Example:
    		Up=328

### [VT numeric keypad] section

In this section, VT numeric keys are assigned to PC keys.

    	Format:
    		<VT numeric key name>=<PC key code>

    	where:

    	  <VT numeric key name>
    		Num0, Num1, Num2, Num3, Num4, Num5, Num6, Num7, Num8,
    		Num9, NumMinus, NumComma, NumPeriod, NumEnter, PF1,
    		PF2, PF3, PF4

    	  <PC key code>
    		PC key code (decimal number)

    	Example:
    		Num0=82

#### 注意

VT 端末ではメインキーパッドの "Enter" キーと数値キーパッドの "Enter" キーが違う文字列を送出するモードがあるので、"NumEnter=" の 後にはメインキーの "Enter" の PC key code を書かないでください。 メインキーパッドの "Enter" と数値キーパッドの "Enter" が同じ PC key code を発生するキーボード(例えば PC9801 キーボード)の場合は 注意が必要です。

### [VT function keys] section

In this section, VT function keys are assigned to PC keys.

    	Format:
    		<VT function key name>=<PC key code>

    	where:

    	  <VT function key name>
    		(Function keys of VT terminal)
    		Hold, Print, Break, F6, F7, F8, F9, F10, F11, F12,
    		F13, F14, Help, Do, F17, F18, F19, F20
    		("User defined keys" of VT terminal)
    		UDK6, UDK7, UDK8, UDK9, UDK10, UDK11, UDK12, UDK13,
    		UDK14, UDK15, UDK16, UDK17, UDK18, UDK19, UDK20

    	  <PC key code>
    		PC key code (decimal number)

    	Example:
    		F6=64

### [X function keys] section

In this section, Xterm F1-F5 keys and BackTab key are assigned to PC keys.

    	Format:
    		<Xterm function key name>=<PC key code>

    	where:

    	  <Xterm function key name>
    		XF1, XF2, XF3, XF4, XF5, XBackTab

    	  <PC key code>
    		PC key code (decimal number)

    	Example:
    		XF1=59

### [Shortcut keys] section

In this section, Tera Term functions are assigned to PC keys.

    	Format:
    		<Shortcut key name>=<PC key code>

    	where:
    	  <Shortcut key name>	Function
    	  --------------------------------------------
    	  EditCopy		[Edit] Copy command
    	  EditPaste		[Edit] Paste command
    	  EditPasteCR		[Edit] Paste<CR> command
    	  EditCLS		[Edit] Clear screen command
    	  EditCLB		[Edit] Clear buffer command
    	  ControlOpenTEK	[Control] Open TEK command
    	  ControlCloseTEK	[Control] Close TEK command
    	  LineUp		Scrolls up screen by 1 line
    	  LineDown		Scrolls down by 1 line
    	  PageUp		Scrolls up by 1 page
    	  PageDown		Scrolls down by 1 page
    	  BuffTop		Scrolls screen to buffer top
    	  BuffBottom		Scrolls screen to buffer bottom
    	  NextWin		Moves to the next Tera Term window
    	  PrevWin		Moves to the previous Tera Term window
    	  NextShownWin		Moves to the next Tera Term window (except minimized)
    	  PrevShownWin		Moves to the previous Tera Term window (except minimized)
    	  LocalEcho		Toggles the local echo status

    	  <PC key code>
    		PC key code (decimal number)

    	Example:
    		LineUp=1352

### [User keys] section

This section defines user keys for functions, sending a character string, executing a macro file or executing a menu command.

    	Format:
    		<User key name>=<PC key code>,<Control flag>,
    				<Character string>

    	where:

    	  <User key name>
    		User1, User2, User3,...., User99
    		Maximum number of user keys is 99.
    		For example, if you want to define ten user keys,
    		you must use the first ten names, from "User1" to "User10".

    	  <PC key code>
    		PC key code (decimal number)

    	  <Control flag>
    		Control flag which specifies how <character string>
    		is treated when the PC key is pressed.
    			0	<Character string> is sent as it is.
    			1	New-line codes in <Character string>
    				are converted by Tera Term and
    				the converted string is sent.
    			2	A macro file which has the name of
    				<Character string> is executed.
    			3	A Tera Term menu command specified
    				by the menu ID <Character string> is
    				executed.

    	  <Character string>
    		If <Control flag> is 0 or 1, <Character string>
    		represents the character string to be sent.
    		A non-printable character (control character) in
    		the string can be expressed as a "$" and ASCII code
    		in two-character hex number. For example, CR character
    		is expressed as "$0D". "$" itself is expressed as "$24".
    		See "Appendix A  ASCII CODE TABLE".

    		If <Control flag> is 2, <Character string> specifies
    		the macro file name to be executed.

    		If <Control flag> is 3, <Character string> is the menu
    		ID which specifies the menu command to be executed.
    		The menu ID should be expressed as a decimal number.
    		See "Appendix B  LIST OF MENU IDs".

    	Example:
    		User1=1083,0,telnet myhost
    		User2=1084,0,$0D$0A
    		User3=1085,1,$0D
    		User4=1086,2,test.ttl
    		User5=1087,3,50110

## NOTE

You can use a PC key code only once in the setup file. If you use a PC key code for multiple key assignments, the warning message "Key code XXX is used more than once" is displayed when the file is loaded by Tera Term. In this case, one of the assignments becomes effective and others are ignored.

If you don't want to assign a key item to any PC key, use the word "off" like the following:

        EditCopy=off

## KEY COMBINATIONS

The following key combinations are acceptable to Tera Term and KEYCODE.EXE:

    	Shift+key
    	Ctrl+key
    	Shift+Ctrl+key
    	Shift+Alt+key
    	Ctrl+Alt+key
    	Shift+Ctrl+Alt+key

Since some combinations (such as Alt+key) are used as shortcut keys of Tera Term and Windows, they don't have PC key codes and can't be specified in the keyboard setup file.

[NOTE] You can specify `Alt+key' combination when Alt key uses meta key. Check `Meta key' under Keyboard of Setup menu. The key code can be obtained by KEYCODE.EXE, unfortunately the key code of `Alt+key' combination can not be obtained. Also, you obtain the key code and add 2048 on the value.

For example, the `V' key code is 47, also `Alt+V' key code is 2095.

    ; Shift + Insert
    EditPaste=850

If you change above entry to `EditPaste=2095', you can paste by using `Alt+V' on condition that Meta key is pass through.

You add in the following entry to [User keys] section in KEYBOARD.CNF if you wan to paster by using `Alt+V' remaining `Shift+Insert' function.

    User1=2095,3,50230

# Q & A

Q. Every time I run Tera Term, the warning message "Key code XXX is used more than once" is displayed.
A. See NOTE.

Q. I want to use the PC "F1" key as the VT100 PF1 key. I edit the keyboard setup file like the following but it does not work:

    	[VT function keys]
    	F1=PF1		(This is wrong.)

A. The left hand side can not be the name of a **PC key** but the name of a **VT terminal key**. The right hand side can not be the name of a key but a PC key code. See "3.1 FORMAT OF THE KEYBOARD SETUP FILE". You should also be careful not to specify a PC key code more than once in the setup file (see "3.2 NOTE").
Edit the keyboard setup file like the following:

    	[VT function keys]
    	PF1=59			(59 is the keycode for the F1 key.)
    	[X function keys]
    	;XF1=59			(Avoid specifying 59 twice.)
    	XF1=off			(Replace 59 by "off".)

Q. How to edit the keyboard setup file to assign the F1 key for sending the escape sequence "ESC [ A"?
A. You can send any character string by using a user key. See FORMAT OF THE KEYBOARD SETUP FILE. You should also be careful not to specify a PC keycode more than once in the setup file (see NOTE).
Edit the keyboard setup file like the following:

    	[X function keys]
    	;XF1=59			(59 is the keycode for the F1 key.)
    					(Avoid specifying 59 twice.)
    	XF1=off			(Replace 59 by "off".)
    	[User keys]
    	User1=59,0,$1B[A		(The ASCII code for ESC is $1B.)