# XMODEM Receive ([File] Transfer menu)

Receives a file from the host with the XMODEM protocol. Activate the send command of the host's XMODEM before executing this command.

## "XMODEM Receive" dialog box

### File Name

Enter the file name to be received.

### Option

Checksum/CRC
  Selects type of error detection(Checksum/CRC).
  Packet size(1K) can be only specified at sender side.
Binary
  - Checkd: Received data is treated as binary and saved in a file without modification.
    The last received packet is packed with padding(EOF,$1A). For this reason, the end of file cannot be known when the end of the sent file is $1A.
  - Unchecked: Received data is treated as text and saved in a file.
    following processes are performed:
    - Newline code conversion
      A single CR($0D) or LF($0A) is converted to CR+LF($0D+$0A).
    - Remove padding(EOF,$0A) of each reciving packet
      EOF($1A) does not appear in the text. So $1A at the end of the file will be removed.

Tips on XMODEM