# Serial port ([Setup] menu)

## "Serial port setup" dialog box

Port
  Serial port to be used.
Baud rate, Data, Parity, Stop, Flow control
  Serial port parameters. Choose the appropriate parameters for the modem or the host.

  The baud rate can be specified with any number. Actually, the serial port driver may not reflect your baud rate.

  Note: If Data is 7 bit, the XMODEM, ZMODEM, B PLUS and Quick-VAN protocols are disabled. If Flow control is Xon/Xoff, the XMODEM and Quick-VAN protocols are disabled.

Transmit delay
  Time intervals between characters (lines) being sent, in milliseconds.