# Serial port ([Setup] menu)

## "Serial port setup" dialog box

OK button
  The label of OK button is changed refering to the connection state.
  Connect with New window ... Serial connection is launched with new window since TCP/IP connection is using.
  New open ... Serial connection starts.
  Close and New open ... Current COM port is closed and serial connection starts with new COM port.
  New setting ... The setting of current COM port is changed.
Cancel button
  Discards the setting change and close the dialog.
Help button
  Displays the help file.
Port
  Serial port to be used. By default, maximum serial port number in the list is 256. It is configurable in MaxComPort setting.
Speed, Data, Parity, Stop bits, Flow control
  Serial port parameters. Choose the appropriate parameters for the modem or the host.

  The Speed can be specified with any number. Actually, the serial port driver may not reflect your speed.

  Flow control can be configured in the following:
  Xon/Xoff ... Software flow
  RTS/CTS ... Hardware flow(RTS/CTS)
  DSR/DTR ... Hardware flow(DSR/DTR)
  none ... No flow control

  Note: If Data is 7 bit, the XMODEM, ZMODEM, B PLUS and Quick-VAN protocols are disabled. If Flow control is Xon/Xoff, the XMODEM and Quick-VAN protocols are disabled.

  Note: The "hardware" prior to version 4.104 applies to RTS/CTS.

Transmit delay
  Time intervals between characters (lines) being sent, in milliseconds.
Detail information of COM port
  The detail information of selected port is shown in the text box.
  You can select all data by using CTRL+A. You can scroll horizontally by using CTRL/SHIFT + wheel.