# sendmulticast

Sends the data to the multicast host.

    sendmulticast <multicastname> <data1> <data2>....

## Remarks

Causes Tera Term to sends characters to the multicast terminal specified by <multicastname> argument or command line option. Beforehand, the name of terminal identification must be configured by using setmulticastname command.
If <data> is a string, the string is sent to the host.
If <data> is an integer, its lowest-order byte (0-255) is regarded as an ASCII code of the character, and the character is sent to the host.

NOTICE: Sent data is ignored on the terminal the AcceptBroadcast is disabled.

## Example

    ; TerminalA
    setmulticastname 'screen1'
    ; Do not receive any strings.

    ; TerminalB
    setmulticastname 'screen2'
    ; The 'violin' string will be sent by the TerminalD.

    ; TerminalC
    setmulticastname 'screen2'
    ; The 'violin' string will be sent by the TerminalD.

    ; TerminalD
    setmulticastname 'screen3'
    sendmulticast 'screen2' 'violin' 13 10     ; Multicast transmission
    ; Do not receive any strings.