# Broadcast command([Control] Menu)

## If "Realtime mode" is off

Command input control
  Input the command to be sent to each window.
Enter key
  Choose an option whether new line is added or not after the transmission of the control command specified in above. A New line code can be chosen from the list of "CRLF", "CR", "LF".
Submit
  Transmit the command. If "AcceptBroadcast" of the window is effective, the command will be received.
History
  Choose an option whether to save the history of transmitted commands. A maximum number of history to be saved can be specified by "MaxBroadcatHistory" .
Send to this process only
  If this option is chosen, the command will be transmitted only to the Tera Term window where "Broadcast command" dialog is specified.
Windows List
  Choose the windows where the commands will be transmitted.

## If "Realtime mode" is on

Command input control
  Keys entered with this control focused will be transmitted to the windows that are chosen in the following window list. The command will be received by the window where "AcceptBroadcast" is even disabled.
Windows List
  Choose the windows where the commands will be transmitted.